Rail Profile Grinding template Ruler

1. Character
The template ruler is an important tool for new standardizing rail grinding works.
It has many characters, such as easy to carry, easy to operate and intelligible etc.
2. Main Technical Parameters
Take template ruler for 60N rail as an example (operational template rulers are provided)
Type: 60N
Number of profile curves: 8
[bookmark: _GoBack]Contrast angle for checking: -5 degree to 60 degree
The 0 degree curve angle for grinding wheel checking and adjusting: 1
Rail gauge for testing: from 1100mm to 1535mm (it will be adjustable)
Over size: 1100 times 35 times 60mm
3. Usage
Adjust the telescopic rod to be suitable for the track gauge, and then place the template ruler on the rail for testing.
After that, an effective grinding operation will be carried out according to the appearance of the shape that does not conform to the profile of template ruler. (Different types of template rulers will be chosen according to the different kinds of grinding requirements)
